**PB-ES(275)**

**Pneumatic power chuck**

* Air chuck for external clamping with built-in pneumatic cylinder.
* Fast and clamping jaw stroke.
* Clamping pressure control.
* Clamping stroke control.





UNIT : mm

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| SPECModel | Through-Hole(mm) | TotalStroke / Jaw(mm) | FastStroke / Jaw(mm) | ClampingStroke / Jaw(mm) | PistonArea(cm2) | OperatingPressureMin.-Max.(bar)  | Gripping\*Force(KN.) | Max.Speed(r.p.m.) | Weight(kg) | MomentOf Inertia I(kg‧m2 ) | Air\*Consumption(L) |
| 600-275 | 275 | 25.4 | 16.9 | 8.5 | 954 | 2-10 | 180 | 1100 | 360 | 20.6 | 39.5 |

\*When operating pressure at 6 bar.