
**F66**

**High speed and light weight type strong finger chuck for aluminum wheel**

* All sliding surfaces are hardened and ground for accurate actual running and long service repeatability.
* Mounting : Adaptor mounting to fit with DIN, ISO, BS, ASA, B5-9 type A spindles.





UNIT : mm

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| SPEC Model | Applicable Wheel Size | Out Dai. Of Chuck (mm) | Available Spindle Nose | Max. Pull Force (kgf) | Max. Gripping Force (kN) | Max. Operating Pressure MPa(kgf/cm2) | Max. Speed (r.p.m.) | Weight (Without Jigs) (kg) | Matching Cylinder |
| F66A8 | 19"-24" | 660 | A2-8 | 3000 | 3300 | 2.9(29.5) | 1500 | 182 | MS125C35 |