**F52**

**High speed and light weight type strong finger chuck for aluminum wheel**

* All sliding surfaces are hardened and ground for accurate actual running and long service repeatability.
* Mounting : Adaptor mounting to fit with DIN, ISO, BS, ASA, B5-9 type A spindles.





UNIT : mm

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| SPECModel | ApplicableWheel Size | Out Dai.Of Chuck(mm) | AvailableSpindle Nose | Max.PullForce(kgf) | Max.GrippingForce(kN) | Max.OperatingPressureMPa(kgf/cm2) | Max.Speed(r.p.m.) | Weight(Without Jigs)(kg) | MatchingCylinder |
| F52A8 | 12"-18" | 521 | A2-8 | 3000 | 3300 | 2.9(29.5) | 2800(18"2200) | 98 | MS125C35 |