
**HB4**

**Boring mill jaw**


* Clamping of workpiece for larger size lathe, vertical lathe, die set with jig.
* One set of 4-piece with T-bolt.






UNIT : mm

|  |  |  |  |
| --- | --- | --- | --- |
| SPEC Model | Jaw Stroke (mm) | Max. Gripping Force (kN) | Weight (kg) |
| HB4-160 | 20 | 39.2 | 29 |



UNIT : mm

|  |  |  |  |
| --- | --- | --- | --- |
| SPEC Model | Jaw Stroke (mm) | Max. Gripping Force (kN) | Weight (kg) |
| HB4-189 | 50 | 39.2 | 31 |



UNIT : mm

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| SPEC Model | Jaw Stroke (mm) | Max. Gripping Force (kN) | Weight (kg) | Matching Soft Jaw |
| HB4-2P | 50 | 39.2 | 31 | HE2486 |