
**PB-ES(375)**

**Pneumatic power chuck**

* Air chuck for external clamping with built-in pneumatic cylinder.
* Fast and clamping jaw stroke.
* Clamping pressure control.
* Clamping stroke control.





UNIT : mm

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| SPEC Model | Through -Hole (mm) | Total Stroke / Jaw (mm) | Fast Stroke / Jaw (mm) | Clamping Stroke / Jaw (mm) | Piston Area (cm2) | Operating Pressure Min.-Max.(bar) | Gripping\* Force (KN.) | Max. Speed (r.p.m.) | Weight (kg) | Moment Of Inertia  I (kg‧m2 ) | Air\* Consumption (L) |
| 850-375 | 375 | 25.4 | 13.4 | 125 | 1342 | 2-10 | 250 | 750 | 980 | 110 | 68 |

\*When operating pressure at 6 bar.