

**P165**

**Floating plate center chuck**

* Suitable for easy one step cutting of thin hores, plate and outside diameter.







UNIT : mm

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| SPEC Model | Plunger Stroke (mm) | Max. Operating Pressure MPa(kgf/cm2) | Max. Speed (r.p.m.) | Weight (kg) | Moment Of Inertia I (kg‧m2 ) | Matching Cylinder |
| P165 | 35 | 1.0(10) | 6000 | 18.5 | 0.02 | MS125C35 |